{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":7,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Temperature Change in degrees Celcius","Thermal Expansion of Carbon Steel m/100m"]
[13.9,1.4999999999999999E-2,null,null,"Temperature Change =",35,"degrees Celcius"]
[27.8,0.03,null,null,"Thermal Expansion =",{"$f":"interpolatetable(A2:A6,B2:B6,F2)","v":3.7769784172661865E-2},"m/100m"]
[41.7,4.4999999999999998E-2]
[55.6,0.06]
[83.3,0.09]